**SPARES AND EQUIPMENT LIST FOR TOURS**

You may wish to carry various spares on tours, but do note that they add weight and bulk in a generally already small packing area. A lot of this should be able to fit in various nooks and crannies around your car. This list is only for guidance and is in no particular order. Please also refer to the national regulations to ensure that you have everything required by law.

* Hi-visability jackets (one for each occupant – must be kept in the car cabin so you can access them without exiting the vehicle)
* Spare bulb kit
* Warning triangle
* Fire extinguisher
* First aid kit
* Tow rope
* Tool kit (general and car specific) (adjustable spanner, socket spanner, screw drivers, long-nosed pliers or fuse removal tool)
* Torch (and batteries)
* Jack and handle (a flat wood base is also useful)
* Spare wheel (check the pressure)
* Spare inner tube(s) – if applicable
* Grease gun
* Bungee cords & cable ties (always useful)
* Spare keys
* Spark plugs
* Fan belts
* Water pump
* Fuel pump
* Fuel filter or funnel with mesh filter
* Fuel pipe/hose and fittings
* Distributor cap and leads
* Rotor arms (several)
* Points and condenser
* Ignition coil
* Relays and fuses (relevant to your vehicle – for fans and fuel pump)
* Oil – if you use 20/50 it is not always readily available from many garages
* WD40, araldite rapid, superglue
* Octane booster (if needed)
* Insulation tape and gaffer/duct tape
* Jubilee clips for hoses
* Electrical cables and connectors
* Wiper blades/arms
* Disposable gloves, hand cleaner, wipes, cloths etc
* Vehicle documents
* Personal and travel documents